{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZQS-BY1"]
[]
[]
[]
[]
["","","","","","AZQS100B7Y1B","AZQS140B7Y1B"]
["Dimensions","Unit","","Height","mm","990","1,430"]
["","","","Width","mm","940","940"]
["","","","Depth","mm","320","320"]
["Weight","Unit","","","kg","82.0","101.0"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-5.0","-5.0"]
["","","","Max.","°CDB","46.0","46.0"]
["","Heating","Ambient","Min.","°CWB","-15.0","-15.0"]
["","","","Max.","°CWB","15.5","15.5"]
["Sound power level","Cooling","","","dBA","70.0","70.0"]
["","Heating","","","dBA","70.0","70.0"]
["Sound pressure level","Cooling","","Nom.","dBA","53","53"]
["","Heating","","Nom.","dBA","57","54"]
["","Night quiet mode","","Level 1","dBA","49","49"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","Charge","","","kg","2.9","4.0"]
["","GWP","","","","2,087.5","2,087.5"]
["Piping connections","Liquid","","OD","mm","9.52","9.52"]
["","Gas","","OD","mm","15.9","15.9"]
["","Piping length","OU - IU","Max.","m","50, 30 (1)","30 (1), 50"]
["","","System","Equivalent","m","70, 40 (1)","40 (1), 70"]
["","","","Chargeless","m","30","30"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","m","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5"]
["Standard Accessories","Tie-wraps","","","","2","2"]
["","Installation manual","","","","1","1"]
["Power supply","Phase","","","","3N~","3N~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","380-415","380-415"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","20","25"]
["Notes","","","","","(1) - For combination with FCAG~AVEB indoor units","(1) - For combination with FCAG~AVEB indoor units"]
["","","","","","(2) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(2) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["","","","","","(4) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(4) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A"]