{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":27,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWAD-TZPSD"]
[]
[]
[]
[]
["","","","","","EWAD960TZPSD2","EWADC12TZPSD2","EWADH11TZPSD2","EWAD615TZPSD2","EWAD810TZPSD2","EWAD405TZPSD1","EWADH14TZPSD2","EWAD530TZPSD2","EWADH15TZPSD2","EWAD370TZPSD1","EWADH10TZPSD2","EWADC10TZPSD2","EWAD285TZPSD1","EWADH13TZPSD2","EWAD450TZPSD1","EWAD575TZPSD2","EWAD890TZPSD2","EWAD675TZPSD2","EWAD330TZPSD1","EWADH12TZPSD2","EWAD735TZPSD2","EWAD490TZPSD1"]
["Cooling capacity","Nom.","","","kW","958.4","1,203","1,137","617.7","809.8","401.5","1,455","529.6","1,568","367.9","1,072","1,003","285.8","1,372","447","571.8","885.5","676.1","330.4","1,298","733.5","486.1"]
["Capacity control","Method","","","","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless"]
["","Minimum capacity","","","%","13","10","11","11","10","30","15","13","14","18","11","12","23","10","28","12","14","10","20","10","10","25"]
["Power input","Cooling","","Nom.","kW","271.7","357.4","325.9","171.1","226.1","105.2","409.5","143.1","462.1","106","312.5","281.9","77.75","409.1","117.3","158.6","242.4","194","92.02","387.4","210.7","130.3"]
["EER","","","","","3.5","3.4","3.5","3.6","3.6","3.8","3.6","3.7","3.4","3.5","3.4","3.6","3.7","3.4","3.8","3.6","3.7","3.5","3.6","3.4","3.5","3.7"]
["IPLV","","","","","6.8","6.7","6.9","6.5","6.8","7.3","6.2","6.7","6.5","6.6","6.7","6.5","6.7","6.6","7.6","6.6","7","6.4","6.7","6.6","6.5","7.5"]
["SEER","","","","","6.602","6.398","6.529","6.28","6.48","6.687","5.978","6.391","5.928","6.389","6.483","6.648","6.29","6.31","6.64","6.301","6.725","6.161","6.465","6.263","6.216","6.567"]
["Dimensions","Unit","","Depth","mm","10,120","12,280","12,280","9,040","10,120","6,880","13,360","7,960","13,360","5,800","11,200","11,200","4,720","13,360","6,880","7,960","10,120","9,040","5,800","12,280","9,040","6,880"]
["","","","Height","mm","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553","2,553"]
["","","","Width","mm","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238","2,238"]
["Weight","Operation weight","","","kg","8,253","9,520","9,515","6,651","7,976","5,163.1","12,021","6,159","12,036","4,354","8,754","8,744","3,863","11,337","5,272.3","6,164","8,243","6,661","4,349","10,846","6,825","5,277.3"]
["","Unit","","","kg","7,642","8,798","8,798","6,311","7,385","5,050","10,805","5,829","10,805","4,256","8,123","8,123","3,775","10,136","5,136","5,829","7,642","6,311","4,256","9,655","6,427","5,136"]
["Casing","Colour","","","","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white","Ivory white"]
["","Material","","","","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet"]
["Water heat exchanger - evaporator","Type","","","","Shell and tube - direct expansion","Shell and tube - direct expansion","Shell and tube - direct expansion","Shell and tube - direct expansion","Shell and tube - direct expansion","Brazed plate","Shell and tube - direct expansion","Shell and tube - direct expansion","Shell and tube - direct expansion","Brazed plate","Shell and tube - direct expansion","Shell and tube - direct expansion","Brazed plate","Shell and tube - direct expansion","Brazed plate","Shell and tube - direct expansion","Shell and tube - direct expansion","Shell and tube - direct expansion","Brazed plate","Shell and tube - direct expansion","Shell and tube - direct expansion","Brazed plate"]
["","Water volume","","","l","481","557","557","255","481","58.1","1,011","255","1,011","48","481","481","48","1,011","76.3","255","481","255","48","1,011","298","76.3"]
["","Water pressure drop","Cooling","Nom.","kPa","45.66","59.5","54.32","31.94","35.19","24.26","47.4","40.2","53.25","22.69","54.163","49.02","14.02","43.31","17.96","45.95","40.37","27.17","18.52","39.81","39.33","20.86"]
["Air heat exchanger","Type","","","","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel","Microchannel"]
["Fan","Quantity","","","","18","22","22","16","18","12","24","14","24","10","20","20","8","24","12","14","18","16","10","22","16","12"]
["","Type","","","","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller","Direct propeller"]
["","Air flow rate","Cooling","Nom.","l/s","101,780","140,200","140,200","90,480","101,780","67,850","152,940","79,170","152,940","56,540","113,080","113,080","45,240","152,940","67,850","79,170","101,780","90,480","56,540","140,200","90,480","67,850"]
["Fan motor","Drive","","","","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless","Brushless"]
["Compressor","Quantity","","","","2","2","2","2","2","1","2","2","2","1","2","2","1","2","1","2","2","2","1","2","2","1"]
["","Type","","","","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor","Screw compressor"]
["Operation range","Air side","Cooling","Min.","°CDB","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46","46"]
["","Water side","Evaporator","Min.","°CDB","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4","4"]
["","","","Max.","°CDB","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18","18"]
["Sound power level","Cooling","","Nom.","dBA","100","105","103","101","105","95","102","100","103","100","102","101","97","106","96","100","99","101","98","108","102","98"]
["Sound pressure level","Cooling","","Nom.","dBA","76","78","77","81","84","74","79","79","80","82","77","77","78","79","75","80","76","83","81","78","83","75"]
["Refrigerant","Type","","","","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a"]
["","GWP","","","","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430"]
["","Charge","","","kg","130","165","160","85","110","55","205","75","220","50","150","140","40","190","60","80","120","95","45","180","100","65"]
["","Circuits","","Quantity","","2","2","2","2","2","1","2","2","2","1","2","2","1","2","1","2","2","2","1","2","2","1"]
["Piping connections","Evaporator water inlet/outlet (OD)","","","","219.1mm","219.1mm","219.1mm","168.3mm","219.1mm","139.7mm","273mm","168.3mm","273mm","88.9mm","219.1mm","219.1mm","88.9mm","273mm","139.7mm","168.3mm","219.1mm","168.3mm","88.9mm","273mm","168.3mm","139.7mm"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400"]
["","Voltage range","","Min.","%","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","%","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10","10"]
["Unit","Starting current","","Max","A","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["","Running current","Cooling","Nom.","A","534","674","627","374","466","233","759","318","837","229","601","555","174","759","249","345","490","414","204","721","442","269"]
["","","","Max","A","672","845","796","468","573","293","1,039","399","1,135","285","761","709","220","951","352","429","616","508","258","893","535","404"]
["","Max unit current for wires sizing","","","A","740","929","876","514","607","322","1,143","439","1,248","310","837","780","242","1,021","388","472","677","559","284","982","585","444"]