{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":5,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60F2VEB / RXS60F4V1B"]
["Cooling capacity","Min.","","kW","1.7"]
["","Max.","","kW","6.5"]
["","Nom.","","kW","6.0 (2)"]
["Space cooling","SEER","","","5.50"]
["","Annual energy consumption","","kWh/a","382"]
["","Capacity","Pdesign","kW","6.00"]
["","Energy efficiency class","","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.00"]
["","SCOP/A","","","3.51"]
["","Energy efficiency class","","","A"]
["","Annual energy consumption","","kWh/a","1,596"]
["Piping connections","Liquid","OD","mm","6.35"]
["","Gas","OD","mm","12.7"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","EER","","","2.91 (1)"]
["","Annual energy consumption","","kWh","1,030"]
["","COP","","","3.21 (1)"]
["","Energy labeling Directive","Cooling","","C"]
["","","Heating","","C"]
["Heating capacity","Nom.","","kW","7.0 (3)"]
["","Min.","","kW","1.7"]
["","Max.","","kW","8.0"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]