{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 2MXM-M9"]
[]
[]
[]
[]
["","","","","FTXM25M2V1B / FTXM42M2V1B / 2MXM50M2V1B9"]
["Cooling capacity","Nom.","","kW","5.0"]
["Space cooling","SEER","","","8.57"]
["","Annual energy consumption","","kWh/a","204"]
["","Capacity","Pdesign","kW","5.00"]
["","Energy efficiency class","","","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.20"]
["","SCOP/A","","","4.65"]
["","Energy efficiency class","","","A++"]
["","Pdh Heating capacity at -10°","","kW","3"]
["","Annual energy consumption","","kWh/a","1,265"]
["Nominal efficiency","Annual energy consumption","","kWh","612"]
["","EER","","","4.09"]
["","COP","","","4.03"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Heating capacity","Min.","","kW","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]