{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 5MXM-N"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 5MXM90N2V1B","FTXM20N2V1B / FTXM20N2V1B / FTXM50N2V1B / 5MXM90N2V1B","FTXM20N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90N2V1B","FTXM20N2V1B / FTXM35N2V1B / FTXM35N2V1B / 5MXM90N2V1B","FTXM25N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90N2V1B","FTXM42N2V1B / FTXM50N2V1B / 5MXM90N2V1B","FTXM20N2V1B / FTXM71N2V1B / 5MXM90N2V1B"]
["Cooling capacity","Nom.","","kW","7.80","8.00","8.00","8.00","8.00","8.00"]
["Space cooling","SEER","","","7.55","7.29","7.17","7.18","7.18","6.85"]
["","Annual energy consumption","","kWh/a","366","387","391","392","391","411"]
["","Capacity","Pdesign","kW","7.80","8.00","8.00","8.00","8.00","8.00"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.46","6.46","5.60","6.46","5.60","5.20"]
["","SCOP/A","","","4.50","4.34","4.35","4.20","4.36","4.21"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","2,010","2,083","1,803","2,152","1,799","1,731"]
["Nominal efficiency","EER","","","4.15","3.82","3.71","3.73","3.72","3.34"]
["","Annual energy consumption","","kWh","940","1,047","1,077","1,073","1,075","1,199"]
["","COP","","","4.58","4.28","4.08","3.99","4.09","3.74"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","10.00","10.00","10.00","10.00","10.00","10.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","","","8.00"]
["Heating capacity","Nom.","","kW","","","","","","","10.00"]
["Nominal efficiency","EER","","","","","","","","","3.33"]
["","COP","","","","","","","","","3.69"]
["","Annual energy consumption","","kWh","","","","","","","1202"]
["","Energy labeling Directive","Cooling","","","","","","","","A"]
["","","Heating","","","","","","","","A"]
["Space cooling","Energy efficiency class","","","","","","","","","A+++"]
["","Capacity","Pdesign","kW","","","","","","","8.00"]
["","SEER","","","","","","","","","6.84"]
["","Annual energy consumption","","kWh/a","","","","","","","410"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","A+"]
["","Capacity","Pdesign","kW","","","","","","","4.50"]
["","SCOP/A","","","","","","","","","4.26"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","3.84"]
["","Annual energy consumption","","kWh/a","","","","","","","1478"]