{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":14,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / 4MXS-F"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / FTXS20K2V1B / FTXS25K2V1B / 4MXS68F3V1B2","FTXS20K2V1B / FTXS20K2V1B / FTXS25K2V1B / 4MXS68F3V1B","FTXS20K2V1B / FTXS25K2V1B / FTXS25K2V1B / 4MXS68F3V1B2","FTXS20K2V1B / FTXS25K2V1B / FTXS25K2V1B / 4MXS68F3V1B","FTXS20K2V1B / FTXS50K2V1B / 4MXS68F3V1B2","FTXS20K2V1B / FTXS50K2V1B / 4MXS68F3V1B","FTXS25K2V1B / FTXS42K2V1B / 4MXS68F3V1B2","FTXS25K2V1B / FTXS42K2V1B / 4MXS68F3V1B","FTXS35K2V1B / FTXS35K2V1B / 4MXS68F3V1B2","FTXS35K2V1B / FTXS35K2V1B / 4MXS68F3V1B"]
["Space cooling","SEER","","","5.49","5.49","5.46","5.46","4.93","4.93","4.96","4.96","4.91","4.91"]
["","Annual energy consumption","","kWh/a","415","415","437","437","483","483","473","473","485","485"]
["","Capacity","Pdesign","kW","6.50","6.50","6.80","6.80","6.80","6.80","6.70","6.70","6.80","6.80"]
["","Energy efficiency class","","","A","A","A","A","B","B","B","B","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","5.05","5.05","5.09","5.09","4.30","4.30","4.42","4.42","4.77","4.77"]
["","SCOP/A","","","3.94","3.94","3.94","3.94","3.83","3.83","3.85","3.85","3.90","3.90"]
["","Energy efficiency class","","","A","A","A","A","A","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","1,794","1,794","1,807","1,807","1,572","1,572","1,606","1,606","1,712","1,712"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]