{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":15,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Sound pressure level","Heating","","High","dBA","40","","","","","","45"]
["","","","Silent operation","dBA","19","","","","","","22"]
["","","","Low","dBA","27","","","","","","33"]
["","Cooling","","Silent operation","dBA","19","","","","","","21"]
["","","","Low","dBA","24","","","","","","33"]
["","","","High","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Cooling","","Nom.","dBA","32","","","","","","39"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1","1","1"]
["","Batteries","","","","2","","2","","2","","2","","2"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2","2"]
["","Titanium apatite photocatalytic air purification filter","","","","2","","2","","2","","2","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Piping connections","Liquid","","OD","mm","6.35","","","","","","6.35"]
["","Gas","","OD","mm","9.5","","","","","","9.5"]
["","Drain","","","","18","","","","","","18"]
["Power input","Cooling","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Heating","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Cooling","","","dBA","58","","","","","","59"]
["","Heating","","","dBA","58","","","","","","59"]
["Dimensions","Unit","","Width","mm","780","","","","","","900"]
["","","","Depth","mm","215","","","","","","215"]
["","","","Height","mm","289","","","","","","298"]
["Casing","Colour","","","","White","","","","","","White"]
["Weight","Unit","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Name","","","","V1","","","","","","V1"]
["","Frequency","","","Hz","50","","","","","","50"]
["","Voltage","","","V","220-240","","","","","","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Power input","Cooling","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Heating","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Casing","Colour","","","","","White","White","White","White","White","","White","White","White"]
["Dimensions","Unit","","Height","mm","","215","289","215","298","215","","215","298","215"]
["","","","Width","mm","","780","780","780","900","900","","900","900","900"]
["","","","Depth","mm","","289","215","289","215","298","","298","215","298"]
["Weight","Unit","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Fan","Air flow rate","Cooling","High","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Medium","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Low","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Silent operation","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Heating","High","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Medium","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Low","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Silent operation","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Sound power level","Cooling","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Heating","","","dBA","","58","58","58","59","59","","59","60","60"]
["Sound pressure level","Cooling","","High","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Medium","dBA","","32","33","33","","37","","39","","40"]
["","","","Low","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Silent operation","dBA","","19","19","19","19","19","","21","23","23"]
["","Heating","","High","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Medium","dBA","","34","34","34","","39","","39","","40"]
["","","","Low","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Silent operation","dBA","","19","19","19","19","19","","22","24","24"]
["Piping connections","Liquid","","OD","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gas","","OD","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Drain","","","","","18","18","18","18","18","","18","18","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","ARC466A9","ARC466A6","ARC466A9"]
["Standard Accessories","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["Power supply","Name","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Phase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Voltage","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Sound pressure level","Cooling","","Nom.","dBA","","","33","","37","","","","40"]
["Fan","Air flow rate","Heating","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Sound pressure level","Heating","","Nom.","dBA","","","34","","39","","","","40"]
["Notes","","","","","","","","","","","(4) - 240V"]