{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FUA71AVEB / RZQSG71L3V1B","FUA71AVEB9 / RZQSG71L3V1B","FUA100AVEB9 / RZQSG100L9V1B","FUA125AVEB / RZQSG125L9V1B","FUA125AVEB9 / RZQSG125L9V1B"]
["Cooling capacity","Nom.","","kW","6.80","6.80","9.50","12.00","12.00"]
["Space cooling","Annual energy consumption","","kWh/a","410","410","593","793","793"]
["","Capacity","Pdesign","kW","6.80","6.80","9.50","12.00","12.00"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.33","6.33","7.60","7.60","7.60"]
["","Annual energy consumption","","kWh/a","2,273","2,273","2,654","2,764","2,764"]
["Nominal efficiency","EER","","","3.21","3.21","3.21","2.65","2.65"]
["","Annual energy consumption","","kWh","1,059","1,059","1,480","2,264","2,264"]
["","COP","","","3.61","3.61","3.61","3.41","3.41"]
["","Energy labeling Directive","Cooling","","A","A","A","D","D"]
["","","Heating","","A","A","A","B","B"]
["Heating capacity","Nom.","","kW","7.50","7.50","10.80","13.50","13.50"]
["Space cooling","SEER","","","5.81","5.81","5.61","5.30","5.30"]
["","Energy efficiency class","","","A+","A+","A+","A","A"]
["Space heating (Average climate)","SCOP/A","","","3.90","3.90","4.01","3.85","3.85"]
["","Energy efficiency class","","","A","A","A+","A","A"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]