{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXUA-A"]
[]
[]
[]
[]
["","","","","","FXUA50AVEB","FXUA71AVEB","FXUA100AVEB","FXUA50AVMB (Archived) (Preliminary)","FXUA71AVMB (Archived) (Preliminary)","FXUA100AVMB (Archived) (Preliminary)"]
["Sound pressure level","Heating","","At high fan speed","dBA","37.0","40.0","47.0","37","40.0","47.0"]
["","","","At low fan speed","dBA","33.0","36.0","40.0","33","36.0","40.0"]
["","","","At medium fan speed","dBA","35.0","38.0","44.0","35","38.0","44.0"]
["","Cooling","","At low fan speed","dBA","33.0","36.0","40.0","33","36.0","40.0"]
["","","","At high fan speed","dBA","37.0","40.0","47.0","37","40.0","47.0"]
["","","","At medium fan speed","dBA","35.0","38.0","44.0","35","38.0","44.0"]
["Refrigerant","GWP","","","","675","675","675","675","675","675"]
["","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.029","0.055","0.117","0.050","0.090","0.200"]
["","Heating","","At high fan speed","kW","0.029","0.055","0.117"]
["Cooling capacity","Total capacity","","At high fan speed","kW","5.6","8.0","11.2","5.6","8.0","11.2"]
["","Nom.","","","kW","5.6","8.0","11.2"]
["Piping connections","Liquid","","OD","mm","6.4","6.4","9.5","6.35","6.35","9.52"]
["","","","Type","","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","12.7","12.7","15.9","12.7","12.7","12.9"]
["","","","Type","","Flare connection","Flare connection","Flare connection"]
["","Drain","","","","VP20","VP20","VP20","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Sound power level","Cooling","","At high fan speed","dBA","55.0","58.0","65.0","55","58","65"]
["Air filter","Type","","","","Resin net","Resin net","Resin net","Resin net with mold resistance","Resin net with mold resistance","Resin net with mold resistance"]
["Dimensions","Unit","","Width","mm","950","950","950","950","950","950"]
["","","","Depth","mm","950","950","950","950","950","950"]
["","","","Height","mm","198","198","198","198","198","198"]
["Casing","Material","","","","Resin","Resin","Resin","Resin","Resin","Resin"]
["","Colour","","","","Fresh White","Fresh White","Fresh White"]
["Weight","Unit","","","kg","27","27","28","26","26","27"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","17.0","22.5","31.0","17","22.5","31.0"]
["","","","At low fan speed","m³/min","13.0","16.0","21.0","13","16.0","21.0"]
["Heating capacity","Total capacity","","At high fan speed","kW","6.3","9.0","12.5","6.3","9.0","12.5"]
["","Nom.","","","kW","6.3","9.0","12.5"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6","6","16","16","16"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220-230","220-240/220-230","220-240/220-230"]
["Notes","","","","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Thermal insulation tube","","","","3","3","3"]
["","Sealing material","","","","4","4","4"]
["","Wire clamp material","","","","10","10","10"]
["","Drain hose","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Washer fixing plate","","","","1","1","1"]
["","Extension auxiliary pipe","","","","1","1","1"]
["","Non woven fabric","","","","1","1","1"]
["","Screws","","","","5","5","5"]
["","Washer","","","","8","8","8"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","(4) - Instead of a fuse, use a circuit breaker","(4) - Instead of a fuse, use a circuit breaker","(4) - Instead of a fuse, use a circuit breaker"]
["","","","","","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA"]
["","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]