{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":16,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CM1."]
[]
[]
[]
[]
["","","","","","JEHCCU0040CM1_","JEHCCU0063CM1_","JEHCCU0095CM1_","JEHCCU0100CM1_","JEHCCU0113CM1_","JEHCCU0140CM1_","JEHCCU0170CM1_","JEHCCU0050CM1_","JEHCCU0051CM1_","JEHCCU0067CM1_","JEHCCU0077CM1_"]
["Refrigerating capacity","Medium temperature","R-407A","Nom","kW","","","","0.80","1.66","1.92","","0.80","","1.07"]
["","","R-134a","Nom","kW","0.59","1.06","1.60","","","","","","0.89","","1.28"]
["","","R-404A","Nom","kW","","","","1.59","1.93","2.42","","1.01","","1.33"]
["","","R-407F","Nom","kW","","","","1.41","1.74","2.08","","0.86","","1.15"]
["Parameters at full load and ambient temp. 43°C","R-407A","Te -10°C","Declared COP (COP3)","","","","","","","1.56","","1.42"]
["","","","Power input (D3)","kW","","","","","","1.15","","0.53"]
["","","","Cooling capacity (P3)","kW","","","","","","1.79","","0.76"]
["","R-134a","Te -10°C","Power input (D3)","kW","0.36","0.62","0.89","","","","","","0.53","","0.71"]
["","","","Declared COP (COP3)","","1.42","1.40","1.50","","","","","","1.40","","1.49"]
["","","","Cooling capacity (P3)","kW","0.51","0.86","1.34","","","","","","0.74","","1.06"]
["","R-407F","Te -10°C","Declared COP (COP3)","","","","","","","1.58","","1.46"]
["","","","Cooling capacity (P3)","kW","","","","","","1.85","","0.79"]
["","","","Power input (D3)","kW","","","","","","1.17","","0.54"]
["","R-404A","Te -10°C","Power input (D3)","kW","","","","0.92","1.07","1.26","","0.63","","0.75"]
["","","","Declared COP (COP3)","","","","","1.44","1.43","1.56","","1.33","","1.42"]
["","","","Cooling capacity (P3)","kW","","","","1.32","1.53","1.96","","0.83","","1.07"]
["Weight","Unit","","","kg","49","57","58","57","58","67","68","49","57","56","58"]
["Parameters at full load and ambient temp. 25°C","R-407A","Te -10°C","Declared COP (COP2)","","","","","1.74","1.90","1.87","","1.69","","1.69"]
["","","","Power input (D2)","kW","","","","0.78","0.91","1.04","","0.48","","0.65"]
["","","","Cooling capacity (P2)","kW","","","","1.35","1.73","1.94","","0.82","","1.09"]
["","R-407F","Te -10°C","Power input (D2)","kW","","","","0.75","0.89","0.97","","0.46","","0.62"]
["","","","Cooling capacity (P2)","kW","","","","1.47","1.85","2.15","","0.89","","1.20"]
["","","","Declared COP (COP2)","","","","","1.95","2.07","2.22","","1.94","","1.94"]
["","R-404A","Te -10°C","Declared COP (COP2)","","","","","2.15","2.24","2.32","","2.21","","2.23"]
["","","","Power input (D2)","kW","","","","0.84","0.99","1.13","","0.51","","0.68"]
["","","","Cooling capacity (P2)","kW","","","","1.81","2.22","2.63","","1.14","","1.52"]
["","R-134a","Te -10°C","Cooling capacity (P2)","kW","0.62","1.18","1.79","","","","","","0.97","","1.44"]
["","","","Declared COP (COP2)","","1.84","2.05","2.30","","","","","","2.01","","2.22"]
["","","","Power input (D2)","kW","0.34","0.58","0.78","","","","","","0.48","","0.65"]
["Refrigerant","GWP Type 5","","","","","","","1,387","1,387","1,387","1,387","1,387","","1,387"]
["","GWP Type 2","","","","","","","2,107","2,107","2,107","","2,107","","2,107"]
["","GWP Type 3","","","","","","","1,825","1,825","1,825","","1,825","","1,825"]
["","GWP","","","","1,430","1,430","1,430","","","","","","1,430","","1,430"]
["","Type 3","","","","","","","R-407F","R-407F","R-407F","","R-407F","","R-407F"]
["","Type 2","","","","","","","R-407A","R-407A","R-407A","","R-407A","","R-407A"]
["","Type 5","","","","","","","R-448A","R-448A","R-448A","R-448A","R-448A","","R-448A"]
["","Type","","","","R-134a","R-134a","R-134a","","","","","","R-134a","","R-134a"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-134a","Te -10°C","Rated COP (COPA)","","1.50","1.77","1.86","","","","","","1.77","","1.85"]
["","","","Rated  cooling capacity (PA)","kW","0.59","1.06","1.60","","","","","","0.89","","1.28"]
["","","","Rated  power input (DA)","kW","0.39","0.60","0.86","","","","","","0.50","","0.70"]
["","R-404A","Te -10°C","Rated  power input (DA)","kW","","","","0.89","1.06","1.18","","0.59","","0.72"]
["","","","Rated  cooling capacity (PA)","kW","","","","1.59","1.93","2.42","","1.01","","1.33"]
["","","","Rated COP (COPA)","","","","","1.79","1.82","2.06","","1.72","","1.84"]
["","R-407F","Te -10°C","Rated COP (COPA)","","","","","1.77","1.85","1.93","","1.77","","1.76"]
["","","","Rated  cooling capacity (PA)","kW","","","","1.41","1.74","2.08","","0.86","","1.15"]
["","","","Rated  power input (DA)","kW","","","","0.79","0.94","1.07","","0.49","","0.65"]
["","R-407A","Te -10°C","Rated  power input (DA)","kW","","","","0.80","0.94","1.11","","0.50","","0.66"]
["","","","Rated COP (COPA)","","","","","1.66","1.78","1.74","","1.59","","1.62"]
["","","","Rated  cooling capacity (PA)","kW","","","","1.33","1.66","1.92","","0.80","","1.07"]
["Power input","Medium temperature","R-134a","Nom","kW","0.39","0.60","0.86","","","","","","0.50","","0.70"]
["","","R-404A","Nom","kW","","","","0.890","1.06","1.18","","0.59","","0.720"]
["","","R-407F","Nom","kW","","","","0.79","0.94","1.07","","0.49","","0.65"]
["","","R-407A","Nom","kW","","","","0.80","0.94","1.11","","0.50","","0.66"]
["COP","Medium temperature","","R-134a","","1.50","1.77","1.86","","","","","","1.77","","1.85"]
["","","","R-407F","","","","","1.77","1.85","1.93","","1.77","","1.76"]
["","","","R-407A","","","","","1.66","1.78","1.74","","1.59","","1.62"]
["","","","R-404A","","","","","1.79","1.82","2.06","","1.72","","1.84"]
["Dimensions","Unit","","Width","mm","876","876","876","876","876","1,101","1,101","876","876","876","876"]
["","","","Depth","mm","430","430","430","430","430","444","444","430","430","430","430"]
["","","","Height","mm","606","606","606","606","606","662","662","606","606","606","606"]
["Casing","Colour","","","","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey"]
["Fan","Type","","","","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases"]