{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG140M7V1B"]
["Sound pressure level","Heating","","Nom.","dBA","","52"]
["","Cooling","","Nom.","dBA","","51"]
["Standard Accessories","Tie-wraps","","","","2","2"]
["","Installation manual","","","","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","LOT10 Energy Label","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","2.53"]
["","GWP","","","","","675"]
["","Charge","","","kg","","3.75"]
["","Type","","","","","R-32"]
["Piping connections","Liquid","","OD","mm","","9.52"]
["","Piping length","OU - IU","Max.","m","","85"]
["","","System","Chargeless","m","","40"]
["","","","Equivalent","m","","100"]
["","Gas","","OD","mm","","15.9"]
["","Level difference","IU - IU","Max.","m","","0.5"]
["","","IU - OU","Max.","m","","30.0"]
["","Additional refrigerant charge","","","kg/m","","See installation manual"]
["Sound power level","Cooling","","","dBA","","70"]
["","Heating","","","dBA","","70 (1)"]
["Dimensions","Unit","","Width","mm","","940"]
["","","","Depth","mm","","320"]
["","","","Height","mm","","1,430"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","92"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","","32"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","","(1) - According to ENER Lot 21"]
["","","","","","","(2) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase."]
["","","","","","","(3) - Ssc: Short-circuit power"]
["","","","","","","(4) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current ≤ 16A per phase."]
["Dimensions","Unit","","Height","mm","990"]
["","","","Width","mm","940"]
["","","","Depth","mm","320"]
["Weight","Unit","","","kg","70"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-20"]
["","","","Max.","°CDB","52"]
["","Heating","Ambient","Min.","°CWB","-20"]
["","","","Max.","°CWB","18.0"]
["Sound power level","Cooling","","","dBA","64"]
["Sound pressure level","Cooling","","Nom.","dBA","46"]
["","Heating","","Nom.","dBA","49"]
["Refrigerant","Type","","","","R-32"]
["","Charge","","","kg","2.95"]
["","GWP","","","","675"]
["","Charge","","","tCO2Eq","1.99"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.9"]
["","Piping length","OU - IU","Max.","m","55"]
["","","System","Equivalent","m","75"]
["","","","Chargeless","m","40"]
["","Additional refrigerant charge","","","kg/m","See installation manual"]
["","Level difference","IU - OU","Max.","m","30.0"]
["","","IU - IU","Max.","m","0.5"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","20"]